# -*- text -*-
#
#	3GPP stuff.
#
#	http://pda.etsi.org/exchangefolder/ts_129061v080300p.pdf
#	ETSI TS 129 061 V8.3.0 (2009-06)
#
#       [wireshark] 2009-07-07:  Updated FreeRadius 2.1.6 dictionary.3gpp
#                                 based upon the above specification.
#
#	$Id: dictionary.3gpp 29038 2009-07-09 15:59:02Z wmeier $
#
VENDOR		3GPP				10415

BEGIN-VENDOR	3GPP

#
#	Most of the 'string' attributes are UTF-8 encoded text.
#	Maybe we want a UTF-8 'type' in the server...
#
ATTRIBUTE	3GPP-IMSI				1	string
ATTRIBUTE	3GPP-Charging-ID			2	integer
ATTRIBUTE	3GPP-PDP-Type				3	integer
ATTRIBUTE	3GPP-Charging-Gateway-Address		4	ipaddr
ATTRIBUTE	3GPP-GPRS-Negotiated-QoS-profile	5	string
ATTRIBUTE	3GPP-SGSN-Address			6	ipaddr
ATTRIBUTE	3GPP-GGSN-Address			7	ipaddr
ATTRIBUTE	3GPP-IMSI-MCC-MNC			8	string
ATTRIBUTE	3GPP-GGSN-MCC-MNC			9	string
ATTRIBUTE	3GPP-NSAPI				10	string
ATTRIBUTE	3GPP-Session-Stop-Indicator		11	octets
ATTRIBUTE	3GPP-Selection-Mode			12	string
ATTRIBUTE	3GPP-Charging-Characteristics		13	string
ATTRIBUTE	3GPP-Charging-Gateway-IPv6-Address	14	ipv6addr
ATTRIBUTE	3GPP-SGSN-IPv6-Address			15	ipv6addr
ATTRIBUTE	3GPP-GGSN-IPv6-Address			16	ipv6addr

#
#    This attribute is really an array of IPv6 addresses.
#    Why the heck couldn't they just send multiple attributes?
#
ATTRIBUTE	3GPP-IPv6-DNS-Servers			17	octets

ATTRIBUTE	3GPP-SGSN-MCC-MNC			18	string
ATTRIBUTE	3GPP-Teardown-Indicator			19	octets

ATTRIBUTE	3GGP-IMEISV				20	octets
ATTRIBUTE	3GPP-RAT-Type				21	integer
ATTRIBUTE	3GPP-User-Location-Info			22	octets
ATTRIBUTE	3GPP-MS-TimeZone			23	octets
ATTRIBUTE	3GPP-Camel-Charging-Info		24	octets
ATTRIBUTE	3GPP-Packet-Filter			25	octets
ATTRIBUTE	3GPP-Negotiated-DSCP			26	integer
ATTRIBUTE	3GPP-Allocate-IP-Type			27	integer

VALUE	3GPP-PDP-Type		IPv4		0
VALUE	3GPP-PDP-Type		PPP		1
VALUE	3GPP-PDP-Type		IPv6		2
VALUE	3GPP-PDP-Type		IPv4v6		3

VALUE	3GPP-RAT-Type		Reserved	0
VALUE	3GPP-RAT-Type		UTRAN		1
VALUE	3GPP-RAT-Type		GERAN		2
VALUE	3GPP-RAT-Type		WLAN		3
VALUE	3GPP-RAT-Type		GAN		4
VALUE	3GPP-RAT-Type		HSPA-Evolution	5
VALUE	3GPP-RAT-Type		IEEE-802-16e	101
VALUE	3GPP-RAT-Type		3GPP2-eHRPD	102
VALUE	3GPP-RAT-Type		3GPP2-HRPD	103
VALUE	3GPP-RAT-Type		3GPP2-1xRTT	104
VALUE	3GPP-RAT-Type		3GPP-EPS	105

VALUE	3GPP-Allocate-IP-Type	Do-Not-Allocate-IPv4-IPv6	0
VALUE	3GPP-Allocate-IP-Type	Allocate-IPv4			1
VALUE	3GPP-Allocate-IP-Type	Allocate-IPv6-Prefix		2
VALUE	3GPP-Allocate-IP-Type	Allocate-IPv4-IPv6-Prefix	3

END-VENDOR    3GPP
