#
# dictionary.patton
#               Dictionary for Patton IADs.
#               Written by Pawel Pierscionek <pawel@voiceworks.pl>
#               based on specifications available from vendor
#
# Version:      @(#)dictionary.patton  1.00  urtho  08-Sep-2006
#  $Id: dictionary.patton 28946 2009-07-06 12:39:58Z wmeier $

VENDOR		Patton				1768

BEGIN-VENDOR	Patton

ATTRIBUTE	Patton-Setup-Time				32	string
ATTRIBUTE	Patton-Connect-Time				33	string
ATTRIBUTE	Patton-Disconnect-Time				34	string
ATTRIBUTE	Patton-Disconnect-Cause				35	integer
ATTRIBUTE	Patton-Disconnect-Source			36	string
ATTRIBUTE	Patton-Called-Unique-Id				48	string
ATTRIBUTE	Patton-Called-IP-Address			49	ipaddr
ATTRIBUTE	Patton-Called-Numbering-Plan			50	string
ATTRIBUTE	Patton-Called-Type-Of-Number			51	string
ATTRIBUTE	Patton-Calling-Unique-Id			80	string
ATTRIBUTE	Patton-Calling-IP-Address			81	ipaddr
ATTRIBUTE	Patton-Calling-Numbering-Plan			82	string
ATTRIBUTE	Patton-Calling-Type-Of-Number			83	string
ATTRIBUTE	Patton-Calling-Presentation-Indicator		88	string
ATTRIBUTE	Patton-Calling-Screening-Indicator		89	string

VALUE	Patton-Disconnect-Cause		Valid-cause-code-not-yet-received				0x00
VALUE	Patton-Disconnect-Cause		Unallocated-runassigned-number					0x01
VALUE	Patton-Disconnect-Cause		No-route-to-specified-transit-network-WAN			0x02
VALUE	Patton-Disconnect-Cause		No-route-to-destination						0x03
VALUE	Patton-Disconnect-Cause		send-special-information-tone					0x04
VALUE	Patton-Disconnect-Cause		misdialled-trunk-prefix						0x05
VALUE	Patton-Disconnect-Cause		Channel-unacceptable						0x06
VALUE	Patton-Disconnect-Cause		Call-awarded-and-being-delivered-in-an-established-channel	0x07
VALUE	Patton-Disconnect-Cause		Prefix-0-dialed-but-not-allowed					0x08
VALUE	Patton-Disconnect-Cause		Prefix-1-dialed-but-not-allowed					0x09
VALUE	Patton-Disconnect-Cause		Prefix-1-dialed-but-not-required				0x0A
VALUE	Patton-Disconnect-Cause		More-digits-received-than-allowed-call-is-proceeding		0x0B
VALUE	Patton-Disconnect-Cause		Normal-call-clearing						0x10
VALUE	Patton-Disconnect-Cause		User-busy							0x11
VALUE	Patton-Disconnect-Cause		No-user-responding						0x12
VALUE	Patton-Disconnect-Cause		no-answer-from-user						0x13
VALUE	Patton-Disconnect-Cause		Call-rejected							0x15
VALUE	Patton-Disconnect-Cause		Number-changed							0x16
VALUE	Patton-Disconnect-Cause		Reverse-charging-rejected					0x17
VALUE	Patton-Disconnect-Cause		Call-suspended							0x18
VALUE	Patton-Disconnect-Cause		Call-resumed							0x19
VALUE	Patton-Disconnect-Cause		Non-selected-user-clearing					0x1A
VALUE	Patton-Disconnect-Cause		Destination-out-of-order					0x1B
VALUE	Patton-Disconnect-Cause		Invalid-number-format-incomplete-number				0x1C
VALUE	Patton-Disconnect-Cause		Facility-rejected						0x1D
VALUE	Patton-Disconnect-Cause		Response-to-STATUS-ENQUIRY					0x1E
VALUE	Patton-Disconnect-Cause		Normal-unspecified						0x1F
VALUE	Patton-Disconnect-Cause		Circuit-out-of-order						0x21
VALUE	Patton-Disconnect-Cause		No-circuit/channel-available					0x22
VALUE	Patton-Disconnect-Cause		Destination-unattainable					0x23
VALUE	Patton-Disconnect-Cause		Degraded-service						0x25
VALUE	Patton-Disconnect-Cause		Network-WAN-out-of-order					0x26
VALUE	Patton-Disconnect-Cause		Transit-delay-range-cannot-be-achieved				0x27
VALUE	Patton-Disconnect-Cause		Throughput-range-cannot-be-achieved				0x28
VALUE	Patton-Disconnect-Cause		Temporary-failure						0x29
VALUE	Patton-Disconnect-Cause		Switching-equipment-congestion					0x2A
VALUE	Patton-Disconnect-Cause		Access-information-discarded					0x2B
VALUE	Patton-Disconnect-Cause		Requested-circuit-channel-not-available				0x2C
VALUE	Patton-Disconnect-Cause		Pre-empted							0x2D
VALUE	Patton-Disconnect-Cause		Precedence-call-blocked						0x2E
VALUE	Patton-Disconnect-Cause		Resource-unavailable-unspecified				0x2F
VALUE	Patton-Disconnect-Cause		Quality-of-service-unavailable					0x31
VALUE	Patton-Disconnect-Cause		Requested-facility-not-subscribed				0x32
VALUE	Patton-Disconnect-Cause		Reverse-charging-not-allowed					0x33
VALUE	Patton-Disconnect-Cause		Outgoing-calls-barred						0x34
VALUE	Patton-Disconnect-Cause		Outgoing-calls-barred-within-CUG				0x35
VALUE	Patton-Disconnect-Cause		Incoming-calls-barred						0x36
VALUE	Patton-Disconnect-Cause		Incoming-calls-barred-within-CUG				0x37
VALUE	Patton-Disconnect-Cause		Call-waiting-not-subscribed					0x38
VALUE	Patton-Disconnect-Cause		Bearer-capability-not-authorized				0x39
VALUE	Patton-Disconnect-Cause		Bearer-capability-not-presently-available			0x3A
VALUE	Patton-Disconnect-Cause		Service-or-option-not-available-unspecified			0x3F
VALUE	Patton-Disconnect-Cause		Bearer-service-not-implemented					0x41
VALUE	Patton-Disconnect-Cause		Channel-type-not-implemented					0x42
VALUE	Patton-Disconnect-Cause		Transit-network-selection-not-implemented			0x43
VALUE	Patton-Disconnect-Cause		Message-not-implemented						0x44
VALUE	Patton-Disconnect-Cause		Requested-facility-not-implemented				0x45
VALUE	Patton-Disconnect-Cause		Only-restricted-digital-information-bearer-capability-is-avail	0x46
VALUE	Patton-Disconnect-Cause		Service-or-option-not-implemented-unspecified			0x4F
VALUE	Patton-Disconnect-Cause		Invalid-call-reference-value					0x51
VALUE	Patton-Disconnect-Cause		Identified-channel-does-not-exist				0x52
VALUE	Patton-Disconnect-Cause		A-suspended-call-exists-but-this-call-identity-does-not		0x53
VALUE	Patton-Disconnect-Cause		Call-identity-in-use						0x54
VALUE	Patton-Disconnect-Cause		No-call-suspended						0x55
VALUE	Patton-Disconnect-Cause		Call-having-the-requested-call-identity-has-been-cleared	0x56
VALUE	Patton-Disconnect-Cause		Called-user-not-member-of-CUG					0x57
VALUE	Patton-Disconnect-Cause		Incompatible-destination					0x58
VALUE	Patton-Disconnect-Cause		Non-existent-abbreviated-address-entry				0x59
VALUE	Patton-Disconnect-Cause		Destination-address-missing-and-direct-call-not-subscribed	0x5A
VALUE	Patton-Disconnect-Cause		Invalid-transit-network-selection-national-use			0x5B
VALUE	Patton-Disconnect-Cause		Invalid-facility-parameter					0x5C
VALUE	Patton-Disconnect-Cause		Mandatory-information-element-is-missing			0x5D
VALUE	Patton-Disconnect-Cause		Invalid-message-unspecified					0x5F
VALUE	Patton-Disconnect-Cause		Mandatory-information-element-is-missing-2			0x60
VALUE	Patton-Disconnect-Cause		Message-type-non-existent-or-not-implemented			0x61
VALUE	Patton-Disconnect-Cause		Message-not-compatible-with-call-state				0x62
VALUE	Patton-Disconnect-Cause		information-element-nonexistant-or-not-implemented		0x63
VALUE	Patton-Disconnect-Cause		Invalid-information-element-contents				0x64
VALUE	Patton-Disconnect-Cause		Message-not-compatible-with-call-state-2			0x65
VALUE	Patton-Disconnect-Cause		Recovery-on-timer-expiry					0x66
VALUE	Patton-Disconnect-Cause		parameter-non-existent-or-not-implemented-passed-on		0x67
VALUE	Patton-Disconnect-Cause		Protocol-error-unspecified					0x6F
VALUE	Patton-Disconnect-Cause		Internetworking-unspecified					0x7F

END-VENDOR	Patton
